
@LANGUAGE
ENGLISH

@VERSION
1.03.00

!==================================================================================================================================

@FIELDS
NAME,DESCRIPTION,ITEM_REP

@ITEM_DF
"ESDS32DCD.HeTwTwLocksClos","TWINLIFT TWISTLOCKS ARE CLOSED","Boolean"

"ESDS32DCD.HeTwTwLocksOpen","TWINLIFT TWISTLOCKS ARE OPEN","Boolean"

"ESDS32DCD.HeAllTwiTwLoClo","ALL TWINLIFT TWISTLOCKS ARE CLOSED","Boolean"

"ESDS32DCD.HeTwinDisplay","TWINLIFT DISPLAY","Boolean"

"ESDS32DCD.KeTwinMode","TWIN MODE","Boolean"

"ESDS32DCD.HeSingleMode","SINGLE MODE","Boolean"

"ESDS32DCD.HeAllTwLoBoxUp","ALL TWISTLOCK BOXES ARE UP","Boolean"

"ESDS32DCD.NsTwinliftSel","TWINLIFT SELECTION TO DISPLAY","Boolean"

"ESDS32DCD.HeAllTwiTwLoOpe","ALL TWINLIFT TWISTLOCKS ARE OPEN","Boolean"

"ESDS32DCD.HeSingleTwinOn","SINGLE TWIN ON","Boolean"

"ESDS32DCD.HeTwLockOpeFr","TWISTLOCKS OPEN (FRONT WHEN TWINLIFT)","Boolean"

"ESDS32DCD.HeTwLockCloFr","TWISTLOCKS CLOSE (FRONT WHEN TWINLIFT)","Boolean"

"ESDS32DCD.HeTwLockCloseRe","TWISTLOCKS CLOSE REAR WHEN TWINLIFT","Boolean"

"ESDS32DCD.HeTwLockOpenRe","TWISTLOCK OPEN REAR WHEN TWINLIFT","Boolean"

"ESDS32DCD.HeAllLandPinsUp","NORMAL & TWINLIFT LANDPINS ARE UP","Boolean"

"ESDS32DCD.HeTwFrontLandPi","TWINLIFT, FRONT CONTAINER LANDPINS ARE UP","Boolean"

"ESDS32DCD.HeTwRearLandPin","TWINLIFT, REAR CONTAINER LANDPINS ARE UP","Boolean"

"ESDS32DCD.HeTwinLiftGapR","GAP BETWEEN TWINLIFT CONTAINERS REAR","Boolean"

"ESDS32DCD.HeSprT_BeLandPiUpFr","SPREADER T-BEAM FRONT LANDPINS ARE UP","Boolean"

"ESDS32DCD.HeSprT_BeLandPiUpRe","SPREADER T-BEAM REAR LANDPINS ARE UP","Boolean"

"ESDS32DCD.HeTwLoOpeFr","TWISTLOCK OPEN FRONT T-BEAM AND TWINLIFT","Boolean"

"ESDS32DCD.HeTwLoCloFr","TWISTLOCK CLOSE FRONT T-BEAM AND TWINLIFT","Boolean"

"ESDS32DCD.HeTwLoCloRe","TWISTLOCK CLOSE REAR T-BEAM AND TWINLIFT","Boolean"

"ESDS32DCD.HeTwLoOpeRe","TWISTLOCK OPEN REAR T-BEAM AND TWINLIFT","Boolean"

"ESDS32DCD.HeTwBoOrLandErFL","TWINLIFT TWISTLOCKBOX/ LANDPIN SENSOR ERROR FRONT LEFT","Boolean"

"ESDS32DCD.HeTwBoOrLandErFR","TWINLIFT TWISTLOCKBOX/ LANDPIN SENSOR ERROR FRONT RIGHT","Boolean"

"ESDS32DCD.HeTwBoOrLandErRL","TWINLIFT TWISTLOCKBOX/ LANDPIN SENSOR ERROR REAR LEFT","Boolean"

"ESDS32DCD.HeTwBoOrLandErRR","TWINLIFT TWISTLOCKBOX/ LANDPIN SENSOR ERROR REAR RIGHT","Boolean"

"ESDS32DCD.HeTwTwLoErrFL","TWINLIFT TWISTLOCK ERROR FRONT LEFT","Boolean"

"ESDS32DCD.HeTwTwLoErrFR","TWINLIFT TWISTLOCK ERROR FRONT RIGHT","Boolean"

"ESDS32DCD.HeTwTwLoErrRL","TWINLIFT TWISTLOCK ERROR REAR LEFT","Boolean"

"ESDS32DCD.HeTwTwLoErrRR","TWINLIFT TWISTLOCK ERROR REAR RIGHT","Boolean"

"ESDS32DCD.HeTwinGapSensEr","TWINLIFT GAP SENSOR ERROR","Boolean"

"ESDS32DCD.HeTwinGapSenErrHoPrev","TWINGAP SENSOR ERROR HOIST PREVENTION WHEN TWLOCKS CLOSED","Boolean"

"ESDS32DCD.KeTwBoxUpFr","TWINLIFT TWISTLOCK BOXES UP FRONT","Boolean"

"ESDS32DCD.KeAutoTwLoBoxUpAllow","AUTOMATIC TWISTLOCK BOXES UP ALLOWED","Boolean"

"ESDS32DCD.POuTwBoxDownL","TWINLIFT TW-LO BOX DOWN LIGHT","Boolean"

"ESDS32DCD.POuTwBoxUpL","TWINLIFT TW-LO BOX UP LIGHT","Boolean"

"ESDS32DCD.HeTwBoxOrLandErr","TWINLIFT TWISTLOCKBOX / LANDPIN ERROR","Boolean"

"ESDS32DCD.HeTwFreeCircVal","TWINLIFT CONTROL FOR FREE CIRC VALVE","Boolean"

"ESDS32DCD.HeOneTwLandPinsUp","AT LEAST ONE OF TWINLIFT LANDPINS ARE UP","Boolean"

"ESDS32DCD.HeOneLandPin","AT LEAST ONE OF LANDPINS ARE ON","Boolean"

"ESDS32DCD.HeHoist5","HELP BIT FOR HOISTING 5 (TWINLIFT)","Boolean"

"ESDS32DCD.HeT_BeLandPinsUp","T-BEAM LANDPINS ARE UP AT SELECTED END (FRONT/REAR) OR AT BOTH END","Boolean"

"ESDS32DCD.HeGap_TwinMode","GAP & TWIN MODE","Boolean"

"ESDS32DCD.HeGap_SingleMod","GAP & SINGLE MODE","Boolean"

"ESDS32DCD.HeNoGap_TwinMod","NO GAP & TWIN MODE","Boolean"

"ESDS32DCD.HeNoGap_SingleM","NO GAP & SINGLE MODE","Boolean"

"ESDS32DCD.KeTwinOnSelect","TWIN ON SELECTION WHEN GAP SENSOR DOESN'T SEE THE GAP","Boolean"

"ESDS32DCD.KeTwinOffSelect","TWIN OFF SELECTION WHEN OPEN TOP CONTAINER","Boolean"

"ESDS32DCD.KeTwinBoxUpRe","TWIN BOX UP REAR","Boolean"

"ESDS32DCD.PInS613TwLoB2CloseFL","TWINLIFT TWISTLOCKS CLOSE B2 FRONT LEFT","Boolean"

"ESDS32DCD.PInS614TwLoB2OpeFL","TWINLIFT TWISTLOCKS OPEN B2 FRONT LEFT","Boolean"

"ESDS32DCD.PInS615TwB2LandPFL","TWINLIFT LANDPINS UP B2 FRONT LEFT","Boolean"

"ESDS32DCD.PInS608TwLoBoUpB1FR","TWISTLOCK BOX B1 UP FRONT RIGHT","Boolean"

"ESDS32DCD.PInS609TwLoB1CloseFR","TWINLIFT TWISTLOCKS CLOSE B1 FRONT RIGHT","Boolean"

"ESDS32DCD.PInS610TwLoB1OpeFR","TWINLIFT TWISTLOCKS OPEN B1 FRONT RIGHT","Boolean"

"ESDS32DCD.PInS611TwB1LandPFR","TWINLIFT LANDPINS B1 UP FRONT RIGHT","Boolean"

"ESDS32DCD.PInS604TwLoBoUpA2RL","TWISTLOCK BOX A2 UP REAR LEFT","Boolean"

"ESDS32DCD.PInS605TwLoA2CloseRL","TWINLIFT TWISTLOCKS CLOSE A2 REAR LEFT","Boolean"

"ESDS32DCD.PInS606TwLoA2OpeRL","TWINLIFT TWISTLOCKS OPEN A2 REAR LEFT","Boolean"

"ESDS32DCD.PInS607TwA2LandPRL","TWINLIFT LANDPINS UP A2 REAR LEFT","Boolean"

"ESDS32DCD.PInS600TwLoBoUpA1RR","TWISTLOCK BOX A1 UP REAR RIGHT","Boolean"

"ESDS32DCD.PInS601TwLoA1CloseRR","TWINLIFT TWISTLOCKS CLOSE A1 REAR RIGHT","Boolean"

"ESDS32DCD.PInS602TwLoA1OpeRR","TWINLIFT TWISTLOCKS OPEN A1 REAR RIGHT","Boolean"

"ESDS32DCD.PInS603TwA1LandPRR","TWINLIFT LANDPINS A1 UP REAR RIGHT","Boolean"

"ESDS32DCD.PInS700_1GapContR","TWINLIFT GAP BETWEEN TWO CONTAINERS  WHEN \"0\", REAR","Boolean"

"ESDS32DCD.PInS702_2TwLiCoFr","TWINLIFT CONTAINERS (NOT TOP OPEN CONTAINER), FRONT","Boolean"

"ESDS32DCD.PInS700_2GapContF","TWINLIFT GAP BETWEEN TWO CONTAINERS  WHEN \"0\", FRONT","Boolean"

"ESDS32DCD.PInS702_1TwLiCoRe","TWINLIFT CONTAINERS (NOT TOP OPEN CONTAINER), REAR","Boolean"

"ESDS32DCD.MachineType","Machine type (1=ESC, 2=ESH, 3=HSC, 4=HSH, 5=FSC, 6=FSH)","UReal"

"ESDS32DCD.MachineNumber","Machine number","UReal"

"ESDS32DCD.EngineHoursTotal","Engine hours (total)","UDReal"

"ESDS32DCD.HybridHoursTotal","Hybrid hours (total)","UDReal"

"ESDS32DCD.TravelingHoursTotalFwd","Traveling hours forward (total)","UDReal"

"ESDS32DCD.TravelingHoursTotalBwd","Traveling hours backward (total)","UDReal"

"ESDS32DCD.HoistLowerTotalHours","Hoisting and Lowering hours (total)","UDReal"

"ESDS32DCD.StandingTotalHours","Standing hours (total)","UDReal"

"ESDS32DCD.TravelingDistanceTotalFwd","Traveling distance forward (total)","UDReal"

"ESDS32DCD.TravelingDistanceTotalBwd","Traveling distance backward (total)","UDReal"

"ESDS32DCD._20ftCountTotal","Number of 20ft containers (total)","UDReal"

"ESDS32DCD._40ftCountTotal","Number of 40ft containers (total)","UDReal"

"ESDS32DCD.TwinCountTotal","Number of twin picks (total)","UDReal"

"ESDS32DCD.FuelConsumptionTotal","Fuel consumption l/h (total)","UReal"

"ESDS32DCD.EnergyConsumptionTotal","Energy consumption kW (total)","UReal"

"ESDS32DCD.NsRPM","RPM TO NS DISPLAY","UReal"

"ESDS32DCD.NsStability","STABILITY TO NS DISPLAY","UReal"

"ESDS32DCD.NsFuelLevelPercentVal","FUEL LEVEL IN % TO DISPLAY","Real"

"ESDS32DCD.ContWeightHex","CONTAINER WEIGHT TO DISPLAY (Tons, HEX)","Real"

"ESDS32DCD.NsEngTemp","ENGINE TEMP TO NS DISPLAY","Real"

"ESDS32DCD.NsSprHeight","SPREADER HEIGHT TO NS DISPLAY","Real"

"ESDS32DCD.NsSprLength","SPREADER LENGTH TO NS DISPLAY","Real"

"ESDS32DCD.NsHoursFwdTrip","FORWARD HOURS (TRIP) FOR NS DISPLAY","UReal"

"ESDS32DCD.NsHoursBwdTrip","BACKWARD HOURS (TRIP) FOR NS DISPLAY","UReal"

"ESDS32DCD.NsHoursInPlaceTrip","IN PLACE HOURS (TRIP) FOR NS DISPLAY","UReal"

"ESDS32DCD.NsKmsFwdTrip","FORWARD KMS (TRIP) FOR NS DISPLAY","UReal"

"ESDS32DCD.NsKmsBwdTrip","REVERSE KMS (TRIP) FOR NS DISPLAY","UReal"

"ESDS32DCD.NsHoistHoursTrip","HOISTING HOURS (TRIP) FOR NS DISPLAY","UReal"

"ESDS32DCD.NsNrOf20contTrip","NUMBER OF 20' CONTAINERS (TRIP) FOR NS DISPLAY","UReal"

"ESDS32DCD.NsNrOf40contTrip","NUMBER OF 40' CONTAINERS (TRIP) FOR NS DISPLAY","UReal"

"ESDS32DCD.NsCentrLub","NUMBER OF CENTRAL LUBRICATIONS FOR NS DISPLAY","Real"

"ESDS32DCD.NsNrOf2x20contTrip","NUMBER OF TWIN / SINGLE LIFTS (TRIP) FOR NS DISPLAY","UReal"

"ESDS32DCD.NsSprLengthFr","SPREADER LENGTH FRONT FOR NS DISPLAY","Real"

"ESDS32DCD.NsSprLengthRe","SPREADER LENGTH REAR FOR DISPLAY","Real"

"ESDS32DCD.NsFuelRate","FUEL RATE l/h FOR NS DISPLAY","Real"

"ESDS32DCD.NsTotFuelUsed","TOTAL FUEL USED FOR NS DISPLAY","UDReal"

"ESDS32DCD.NsFuelConsLTim","ENGINE FUEL CONSUMPTION LONG TIME l/h FOR NS DISPLAY","UReal"

"ESDS32DCD.NsEngineHoursTrip","ENGINE HOURS (TRIP) FOR NS DISPLAY","UReal"
